**Windows Machines 802.1x Manual Configuration**

The wired AutoConfig service must be started and set to Automatic.

Without this service started, the Authentication Tab will not be visible on the Local Area Connection properties.

wired_service.JPG

Next go to the Local Area Connection under Control Panel ->Network and Internet->Network Connections. Right click and go to properties.

On the Authentication Tab, ensure the selections are identical to the screenshot below.  
  
  
