|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Adaptive Radio Management (ARM) Profile >** | |  |  |  | | --- | --- | --- | |  |  |  | |
| * [Basic](javascript:void(0);) * [Advanced](javascript:void(0);)  |  |  | | --- | --- | | Assignment |  | | Allowed bands for 40MHz channels |  | | 80MHz support |  | | 160MHz-support |  | | Client Aware |  | | Max Tx EIRP |  | | Min Tx EIRP |  | | Rogue AP Aware |  | | Active Scan |  | | ARM Over the Air Updates |  | | Scanning |  | | Multi Band Scan |  | | VoIP Aware Scan |  | | Power Save Aware Scan |  | | Video Aware Scan |  | | Ideal Coverage Index |  | | Acceptable Coverage Index |  | | Free Channel Index |  | | Interfering AP Weight | |  |  | | --- | --- | | % |  | | | Backoff Time | |  |  | | --- | --- | | sec |  | | | Error Rate Threshold | |  |  | | --- | --- | | % |  | | | Error Rate Wait Time | |  |  | | --- | --- | | sec |  | | | Channel Quality Aware Arm |  | | Channel Quality Threshold | |  |  | | --- | --- | | % |  | | | Channel Quality Wait Time | |  |  | | --- | --- | | sec |  | | | Minimum Scan Time |  | | Load aware Scan Threshold | |  |  | | --- | --- | | Bps |  | | | Mode Aware Arm |  | | Scan Mode |  | | Client Match |  | | | |

**Adaptive Radio Management (ARM) Profile > **

|  |  |  |
| --- | --- | --- |
|  |  |  |

* [Basic](javascript:void(0);)
* [Advanced](javascript:void(0);)

|  |  |
| --- | --- |
| Assignment |  |
| Allowed bands for 40MHz channels |  |
| 80MHz support |  |
| 160MHz-support |  |
| Client Aware |  |
| Max Tx EIRP |  |
| Min Tx EIRP |  |
| Rogue AP Aware |  |
| Active Scan |  |
| ARM Over the Air Updates |  |
| Scanning |  |
| Multi Band Scan |  |
| VoIP Aware Scan |  |
| Power Save Aware Scan |  |
| Video Aware Scan |  |
| Ideal Coverage Index |  |
| Acceptable Coverage Index |  |
| Free Channel Index |  |
| Interfering AP Weight | |  |  | | --- | --- | | % |  | |
| Backoff Time | |  |  | | --- | --- | | sec |  | |
| Error Rate Threshold | |  |  | | --- | --- | | % |  | |
| Error Rate Wait Time | |  |  | | --- | --- | | sec |  | |
| Channel Quality Aware Arm |  |
| Channel Quality Threshold | |  |  | | --- | --- | | % |  | |
| Channel Quality Wait Time | |  |  | | --- | --- | | sec |  | |
| Minimum Scan Time |  |
| Load aware Scan Threshold | |  |  | | --- | --- | | Bps |  | |
| Mode Aware Arm |  |
| Scan Mode |  |
| Client Match |  |