(ArubaMaster) #show log system 50

Jun 5 15:42:45 KERNEL: 0:<6>usb 1-1: configuration #1 chosen from 1 choice

Jun 5 15:42:45 KERNEL: 0:<6>hub 1-1:1.0: USB hub found

Jun 5 15:42:45 KERNEL: 0:<6>hub 1-1:1.0: 4 ports detected

Jun 5 15:42:45 KERNEL: 0:<6>drivers/usb/class/usblp.c: v0.13: USB Printer Devi ce Class driver

Jun 5 15:42:45 KERNEL: 0:<6>Initializing USB Mass Storage driver...

Jun 5 15:42:45 KERNEL: 0:<6>USB Mass Storage support registered.

Jun 5 15:42:45 KERNEL: 0:Intializing BK-3220 I2C Host Adapter...0:done.

Jun 5 15:42:45 KERNEL: 0:i2c-palm-bk3220: Added I2C Bus 0

Jun 5 15:42:45 KERNEL: 0:Intializing BK-3220 I2C Host Adapter...0:done.

Jun 5 15:42:45 KERNEL: 0:i2c-palm-bk3220: Added I2C Bus 1

Jun 5 15:42:45 KERNEL: 0:<6>i2c-grenache: using default base 0xbd000000

Jun 5 15:42:45 KERNEL: 0:Registering powr6at6 I2C Power Trim Controller driver

Jun 5 15:42:45 KERNEL: 0:Found POWR6AT6 on Palm Chip BK3220 Adapter 0

Jun 5 15:42:45 KERNEL: 0:Found POWR6AT6 on Grenache I2C\_0

Jun 5 15:42:45 KERNEL: 0:Registering max6640 I2C based Temperature Sensor driv er...

Jun 5 15:42:45 KERNEL: 0:Found MAX6640 on Grenache I2C\_0

Jun 5 15:42:45 KERNEL: 0:Registering Phoenix I2C based RTC driver...

Jun 5 15:42:45 KERNEL: 0:<6>: Found DS1374 on Palm Chip BK3220 Adapter 0

Jun 5 15:42:45 KERNEL: 0:Registering Phoenix I2C based TPM driver...

Jun 5 15:42:45 KERNEL: 0:Registering Broadcom I2C POE driver...

Jun 5 15:42:45 KERNEL: 0:<6>: Found BCM59103 on Grenache I2C\_0

Jun 5 15:42:45 KERNEL: 0:<6>: Found BCM59103 on Grenache I2C\_1

Jun 5 15:42:45 KERNEL: 0:<6>802.1Q VLAN Support v1.8 Ben Greear <greearb@cande latech.com>

Jun 5 15:42:45 KERNEL: 0:<6>All bugs added by David S. Miller <davem@redhat.co m>

Jun 5 15:42:45 KERNEL: 0: ^H1:flushing more than page size of icache addresses starting @ c00c1000

Jun 5 15:42:45 KERNEL: 1:<6>drivers/usb/serial/usb-serial.c: USB Serial suppor t registered for generic

Jun 5 15:42:45 KERNEL: 1:<6>drivers/usb/serial/usb-serial.c: USB Serial Driver core

Jun 5 15:42:45 KERNEL: 0:flushing more than page size of icache addresses star ting @ c00b9000

Jun 5 15:42:45 KERNEL: 0:<6>drivers/usb/serial/usb-serial.c: USB Serial suppor t registered for GSM modem (1-port)

Jun 5 15:42:45 KERNEL: 0:<6>drivers/usb/serial/option.c: USB Driver for GSM mo dems: v0.7.1

Jun 5 15:42:45 KERNEL: 2:flushing more than page size of icache addresses star ting @ c00b5000

Jun 5 15:42:45 KERNEL: 2:<4>sierra: Ignoring new-style parameters in presence of obsolete ones

Jun 5 15:42:45 KERNEL: 2:<6>drivers/usb/serial/usb-serial.c: USB Serial suppor t registered for Sierra USB modem

Jun 5 15:42:45 KERNEL: 2:<6>drivers/usb/serial/sierra.c: USB Driver for Sierra Wireless USB modems: v.1.2.7

Jun 5 15:42:45 KERNEL: 1:flushing more than page size of icache addresses star ting @ c00d9000

Jun 5 15:42:45 KERNEL: 1:<4>hso: Ignoring new-style parameters in presence of obsolete ones

Jun 5 15:42:45 KERNEL: 1:<6>hso: drivers/usb/serial/hso.c: 1.2 Option Wireless

Jun 5 15:42:45 KERNEL: 1:<6>hso: Registering procfs

Jun 5 15:42:45 KERNEL: cess `syslogd' is using obsolete setsockopt SO\_BSDCOMPA T

Jun 5 15:42:45 KERNEL: 1:<5>JFFS2 notice: (871) check\_node\_data: wrong data CR C in data node at 0x074ea800: read 0xe2a95a29, calculated 0x4118a53d.

Jun 5 15:42:45 KERNEL: 1:<5>JFFS2 notice: (871) check\_node\_data: wrong data CR C in data node at 0x06e48800: read 0x803aa4d4, calculated 0x45c0502f.

Jun 5 15:42:45 KERNEL: 0:<4>process `soed' is using obsolete setsockopt SO\_BSD COMPAT

Jun 5 15:42:46 :314800: <ERRS> |fpapps| NVRAM checksum error detected

Jun 5 15:42:47 :399816: <ERRS> |fpapps| poe download start

Jun 5 15:43:27 :313256: <WARN> |fpapps| Route resolve returned an Error

Jun 5 15:43:30 :306510: <WARN> |publisher| Dropping message from 8214 for serv ice 'aaa-idle-user-timeout (service not found)'

Jun 5 15:43:32 KERNEL: 1:<4>process `snmpd' is using obsolete setsockopt SO\_BS DCOMPAT

Jun 5 15:43:34 KERNEL: 1:<4>process `trapd' is using obsolete setsockopt SO\_BS DCOMPAT

Jun 5 15:43:35 :325022: <ERRS> |authmgr| Bogus VLAN ID:4095 received.

Jun 5 15:43:45 :304001: <ERRS> |stm| Unexpected stm (Station managment) runtim e error at data\_path\_handler, 649, data\_path\_handler: recv - Network is down